**ETS de-activates on its own**

As a workaround to this problem, please follow instructions given below:

* When ETS gets disabled inadvertently, blue LED will be OFF on **QX Tool** back cap. Please look out for blue LED status during fastening operation, especially for Torque strategy when ETS functionality is expected.
* **Enable ETS from tool display/back cap** :
* With help of down arrow button on tool back cap, scroll to screen with “0000” and select ✔



* Enter password as “FFFF” and select ✔



* With help of right arrow button on tool, enter configuration selection screen.



* Select Up arrow button on tool back cap to scroll to ETS selection screen.




* To enable ETS, scroll to rectangular waveform (with increasing amplitude), and select ✔ on tool.




* ETS enabled tool display:




* ETSparameter selection such as Ergonomics, Performance and Productivity modes cannot be configured from QXTool back cap.Use ICS software to make these selections.
* **‘Enable ETS’ setting from ICS software:**
* Select **QX Series** on the home screen



* Select **General Setup** from **Setup** menu



* Turn on the checkbox for **Enable ETS** and save settings.



Note: This is a temporary solution to notify user if ETS gets disabled on its own. This applies to QXX, QXC and QXN tools.